# 🎯 Calibration Suite for Neptune 4 Plus with Cartographer

## Installation

1. Copy all `.cfg` files to your Klipper config directory
2. Add `[include calibration/*.cfg]` to your `printer.cfg`
3. Restart Klipper
4. Run `CALIBRATION_MENU` to start

---

## Macros Overview

- `CALIBRATION_MENU` - Main menu with all options
- `CALIBRATE_Z_OFFSET` - Cartographer Z0 calibration
- `CALIBRATE_INPUT_SHAPER` - ADXL resonance measurement
- `CALIBRATE_PRESSURE_ADVANCE` - PA tuning
- `CALIBRATE_FLOW_RATE` - Flow rate calibration
- `CALIBRATE_TEMPERATURE` - Temperature tower
- `CALIBRATE_RETRACTION` - Retraction tuning
- `CALIBRATE_BED_MESH` - Bed mesh verification
- `CALIBRATION_FULL` - Run all calibrations in sequence

---

## Quick Start

```gcode
; In Mainsail Console or Fluidd Console:
CALIBRATION_MENU
```

---

## Notes

- All macros use Cartographer for precise measurements
- Results are automatically saved with `SAVE_CONFIG`
- Each macro includes safety checks and clear instructions
- Designed for both Original and Bambu Lab hotends
